//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//

.Set READY_VAR = 01


Command ID:	DPMR_CC
Send	Command: 84 A9 61 00 04 03 5C 77 F5 D5
Receive	Command:84 A9 61 00 02 03 5C 00
Command ID: WORK_MODE_DUPLEX
Send command: 84 A9 61 00 04 00 18 03 00 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: PROCESS_MODE
Send command: 84 A9 61 00 02 00 1A 83
//Send command: 84 A9 61 00 02 00 1A 04
Receive Data: 84 A9 61 00 02 00 1A 00
Command ID:	ADDRESSING_MODE
Send	Command: 84 A9 61 00 02 03 28 01
Receive	Command:84 A9 61 00 02 03 28 00
Command ID: DPMR_HT_CI
Send command: 84 A9 61 00 03 03 57 00 00
Receive Data: 84 A9 61 00 02 03 57 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 03 52 12 34 56 70
Receive Data: 84 A9 61 00 02 03 52 00
Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 12 34 56 70
Receive Data: 84 A9 61 00 02 03 53 00
Command ID:	REPORT_FIELD
Send	Command: 84 A9 61 00 02 00 1D ff
Receive	Command:84 A9 61 00 02 00 1D 00
Command ID:	DEMOD_GAIN
Send	Command: 84 A9 61 00 03 00 1C 00 00
Receive	Command:84 A9 61 00 02 00 1C 00

Command ID:	SCRAMBLER_SEED1
Send	Command: 84 A9 61 00 06 00 2A 01 12 34 45 78
Receive	Data:84 A9 61 00 02 00 2A 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 1a
Receive	Command:84 A9 61 00 02 00 20 00
Receive	Data:84 A9 61 00 02 30 1B 09
Receive	Data:84 A9 61 00 02 30 1B 04
Receive Data: 84 A9 61 00 03 30 57 00 00
Receive Data: 84 A9 61 00 02 30 54 1a
Receive Data: 84 A9 61 00 04 30 50 1B 91 FD
Receive Data: 84 A9 61 00 04 30 51 1B 91 FD
Receive	Command:84 A9 61 00 05 30 52 12 34 56 70
Receive	Command:84 A9 61 00 05 30 53 12 34 56 70
Receive	Command:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Command:84 A9 61 00 02 30 27 00
Pause 5000



Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
Receive	Command:84 A9 61 00 02 00 21 00 
Receive	Command:84 A9 61 00 02 20 17 0A
Receive	Command:84 A9 61 00 04 30 4B 00 00 00
Pause 1000


Command ID:	SCRAMBLER_SEED2
Send	Command: 84 A9 61 00 0A 00 2A 02 12 34 45 78 9A BC DE F0
Receive	Data:84 A9 61 00 02 00 2A 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 1a
Receive	Command:84 A9 61 00 02 00 20 00
Receive	Data:84 A9 61 00 02 30 1B 09
Receive	Data:84 A9 61 00 02 30 1B 04
Receive Data: 84 A9 61 00 03 30 57 00 00
Receive Data: 84 A9 61 00 02 30 54 1a
Receive Data: 84 A9 61 00 04 30 50 1B 91 FD
Receive Data: 84 A9 61 00 04 30 51 1B 91 FD
Receive	Command:84 A9 61 00 05 30 52 12 34 56 70
Receive	Command:84 A9 61 00 05 30 53 12 34 56 70
Receive	Command:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Command:84 A9 61 00 02 30 27 00
Pause 5000



Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
Receive	Command:84 A9 61 00 02 00 21 00 
Receive	Command:84 A9 61 00 02 20 17 0A
Receive	Command:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID:	SCRAMBLER_SEED3
Send	Command: 84 A9 61 00 1A 00 2A 03 12 34 45 78 9A BC DE F0 00 11 22 33 44 55 66 77 88 99 AA BB CC DD EE FF
Receive	Data:84 A9 61 00 02 00 2A 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 1a
Receive	Command:84 A9 61 00 02 00 20 00
Receive	Data:84 A9 61 00 02 30 1B 09
Receive	Data:84 A9 61 00 02 30 1B 04
Receive Data: 84 A9 61 00 03 30 57 00 00
Receive Data: 84 A9 61 00 02 30 54 1a
Receive Data: 84 A9 61 00 04 30 50 1B 91 FD
Receive Data: 84 A9 61 00 04 30 51 1B 91 FD
Receive	Command:84 A9 61 00 05 30 52 12 34 56 70
Receive	Command:84 A9 61 00 05 30 53 12 34 56 70
Receive	Command:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Command:84 A9 61 00 02 30 27 00
Pause 5000



Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
Receive	Command:84 A9 61 00 02 00 21 00 
Receive	Command:84 A9 61 00 02 20 17 0A
Receive	Command:84 A9 61 00 04 30 4B 00 00 00
Pause 1000


Command ID:	SCRAMBLER_SEED0
Send	Command: 84 A9 61 00 02 00 2A 00
Receive	Data:84 A9 61 00 02 00 2A 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 1a
Receive	Command:84 A9 61 00 02 00 20 00
Receive	Data:84 A9 61 00 02 30 1B 09
Receive	Data:84 A9 61 00 02 30 1B 04
Receive Data: 84 A9 61 00 03 30 57 00 00
Receive Data: 84 A9 61 00 02 30 54 1a
Receive Data: 84 A9 61 00 04 30 50 1B 91 FD
Receive Data: 84 A9 61 00 04 30 51 1B 91 FD
Receive	Command:84 A9 61 00 05 30 52 12 34 56 70
Receive	Command:84 A9 61 00 05 30 53 12 34 56 70
Receive	Command:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Command:84 A9 61 00 02 30 27 00
Pause 5000



Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
Receive	Command:84 A9 61 00 02 00 21 00 
Receive	Command:84 A9 61 00 02 20 17 0A
Receive	Command:84 A9 61 00 04 30 4B 00 00 00
Pause 1000



