**Firmware V02.03**  
1. Revise the display “UTC” of time zone instead of “UCT”  
Note: V02.03 doesn’t support 120K contacts import, with spare memory for your other DIY requirements.  
  
**Firmware V02.03 (CSV)-V02.03**  
1. Revise the display “UTC” of time zone instead of “UCT”  
Note: V02.03 (CSV) supports 120K contacts import.